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	DEQ AIR QUALITY PROGRAM 

1410 N. Hilton, Boise, ID  83706

For assistance, call the 
Air Permit Hotline – 1-877-5PERMIT
	Cabinet Making Exemption - Form CM-EXPT
Revision 1
11/13/2023


Please see instructions on pages 5-6 before filling out the form.
This form is for cabinetmaking facilities and other small woodworking shops desiring an exemption from the requirement to obtain a Permit to Construct (PTC) for sources of air emissions. The Rules for the Control of Air Pollution in Idaho (IDAPA 58.01.01.220 through 223) allow for owners or operators to exempt certain sources of air emissions from the requirement to obtain a PTC. This form is to be used to help facilities determine whether they are permit exempt and, if so, identify what documentation must be maintained to document the exemption. This form may be used to document a self-exemption analysis or may be submitted to DEQ for an exemption concurrence (at no cost to the Applicant).
Note: For existing sources of air emissions, removal of equipment that generates air emissions cannot be used to offset the increase in air emissions for the equipment or activity for which a PTC exemption is desired.
Additional Note: A PTC exemption does not release the owner or operator of sources of air emissions from compliance with all other applicable federal (e.g., NSPS requirements, Tier I operating permit), state, or local laws, regulations, permits, or ordinances.
Additional Note:  This exemption is not intended to be used at sources located at an existing major facility.  In these instances, a facility should use the Form EXPT to document an individual exemption.
	IDENTIFICATION

	1. Company Name
	2. Facility Name:

	     
	     

	3. Facility ID Number (if applicable)
	4. Primary NAICS Code:

	     
	     

	5.
Project Description (provide a complete description of the equipment or activity being exempted):
	     

	GENERAL INFORMATION

	6.
Facility Information:
	7.
Permitting Contact: 
     
 
8. Telephone No.: 
     

9.
E-mail: 
     

10.
Physical Address: 
     

11.
Mailing Address: 
     



     


     


	12. 
Will you utilize a Level I or Level II Exemption? (see note below)
	 FORMCHECKBOX 
 Level I  go to question 13
 FORMCHECKBOX 
 Level II  go to question 19

	A Level I exemption should be used by most facilities.  This option provides greater flexibility for coating and heater usage.
A Level II exemption may be beneficial for your facility if you intend to use coating materials that contain Carbon Black, Chromium III, or Silica Quartz.  In this case, a Level II exemption will allow increased usage of coatings that contain these substances, but reduced usage for coatings that contain benzene or formaldehyde, and less flexibility regarding heater usage.

	LEVEL I EXEMPTION

	13.
Will the use of all coating materials exceed 3 gallons per day, excluding coatings described in Question 14a?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	14a.
Do any coating materials contain Benzene, Formaldehyde, Carbon Black, Chromium III, or Silica Quartz?
	 FORMCHECKBOX 
 Yes

 FORMCHECKBOX 
 No, go to question 15

	14b.
If so, will usage of these coatings exceed the following amounts?


For coatings that contain Benzene: 
450 gallons per year


For coatings that contain Formaldehyde: 
300 gallons per year


For coatings that contain Carbon Black: 
2.8 gallons per day


For coatings that contain Chromium III: 
0.40 gallons per day


For coatings that contain Silica Quartz: 
0.19 gallons per day
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	15. 
Do any coating materials contain naphthalene?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	16. 
Will all spray coating activities take place in an enclosed booth equipped with a filter system that achieves a 98% control efficiency for PM10/PM2.5


AND


Will all spray coatings be applied using HVLP spray guns (or equivalent) that achieve 65% transfer efficiency?
	 FORMCHECKBOX 
 Yes

 FORMCHECKBOX 
 No  Note: The project cannot be exempted.

	17a.
Will space heaters, furnaces, or commercial boilers be used for heating?
	 FORMCHECKBOX 
 Yes

 FORMCHECKBOX 
 No, go to question 18

	17b.
If space heaters, furnaces, or commercial boilers will be used, what kind of fuels will they burn?
	 FORMCHECKBOX 
 All are electric, go to question 18
 FORMCHECKBOX 
 Natural gas/LPG only, go to question 17c
 FORMCHECKBOX 
 Diesel only, go to question 17d
 FORMCHECKBOX 
 Both natural gas/LPG and diesel, go to question 17e

	17c. 
For the scenario involving only natural gas/LPG-fired heaters/furnaces/boilers, will the total heat input exceed 1.25 MMBtu/hr?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No, go to question 18

	17d.
For the scenario involving only diesel-fired heaters/furnaces/boilers, will the total heat input exceed 0.35 MMBtu/hr?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No, go to question 18

	17e.
For the scenario involving a combination of natural gas/LPG and diesel-fired heaters/furnaces/boilers, will the total heat input of all natural gas/LPG-fired units exceed 0.50 MMBtu/hr and will the total heat input of all diesel-fired units exceed 0.30 MMBtu/hr?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	18. Will saw and sander dust generated at this facility be controlled by individual dust collection systems and/or by a shop dust collector with combined control efficiency of 98% or greater for PM10/PM2.5?
	 FORMCHECKBOX 
 Yes, go to question 31
 FORMCHECKBOX 
 No  Note: The project cannot be exempted.

	LEVEL II EXEMPTION

	19.
Will the use of all coating materials exceed 3 gallons per day, excluding coatings described in Questions 20a and 24?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	20a.
Do any coating materials contain Benzene, Carbon Black, Chromium III, or Silica Quartz?
	 FORMCHECKBOX 
 Yes

 FORMCHECKBOX 
 No, go to question 21

	20b.
If so, will usage of these materials exceed the following amounts?


For coatings that contain Benzene: 
44 gallons per year


For coatings that contain Carbon Black: 
3.0 gallons per day


For coatings that contain Chromium III: 
2.0 gallons per day


For coatings that contain Silica Quartz: 
0.9 gallons per day
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	21. 
Do any coating materials contains naphthalene?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	22. 
Will all spray coating activities take place in an enclosed booth equipped with a filter system that achieves a 98% control efficiency for PM10/PM2.5


AND


Will all spray coatings be applied using HVLP spray guns (or equivalent) achieving 65% transfer efficiency?
	 FORMCHECKBOX 
 Yes

 FORMCHECKBOX 
 No  Note: The project cannot be exempted.

	23.
Will space heaters, furnaces, or commercial boilers be used for heating?
	 FORMCHECKBOX 
 Yes, go to question 25
 FORMCHECKBOX 
 No

	24. 
Will usage of coating materials containing formaldehyde exceed 42 gallons per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No, go to question 30

	25.
If space heaters, furnaces, or boilers will be used, what kind of fuels will they burn?
	 FORMCHECKBOX 
 All are electric, go to question 26
 FORMCHECKBOX 
 Natural gas/LPG only, go to question 27a

 FORMCHECKBOX 
 Diesel only, go to question 28a

 FORMCHECKBOX 
 Both natural gas and diesel, go to question 29a

	Electric Heaters/Furnaces/Boilers Only

	26.
Will usage of coating materials containing formaldehyde exceed 42 gallons per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No, go to question 30


	Natural Gas/LPG-Fired Heaters/Furnaces/Boilers Only

	27a.
Will the total heat input exceed 0.33 MMBtu/hr?
	 FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No, go to question 27c

	27b.
Will the total heat input exceed 1.40 MMBtu/hr


AND


Will operation of any of these exceed 2,080 hours per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	27c.
Will the use of all formaldehyde containing spray coatings exceed 21 gallons per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No, go to question 30

	Diesel-Fired Heaters/Furnaces/Boilers Only

	28a.
Will the total heat input exceed 0.04 MMBtu/hr?
	 FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No, go to question 28c

	28b.
Will the total heat input exceed 0.15 MMBtu/hr


AND


Will operation of any of these exceed 2,080 hours per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	28c.
Will the use of all formaldehyde containing spray coatings exceed 35 gallons per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No, go to question 30

	Both Natural Gas/LPG and Diesel Heaters/Furnaces/Boilers

	29a.
Will the total heat input heat input of all natural gas/LPG-fired units exceed 0.12 MMBtu/hr


AND


Will the total heat input of all diesel-fired units exceed 0.03 MMBtu/hr?
	 FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No, go to question 29c

	29b.
Will the total heat input of all natural gas/LPG-fired units exceed 0.50 MMBtu/hr


AND


Will the total heat input of all diesel-fired units exceed 0.13 MMBtu/hr


AND


Will the operation of any of these units exceed 2,080 hours per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	29c. 
Will the use of all formaldehyde containing spray coatings exceed 29 gallons per year?
	 FORMCHECKBOX 
 Yes  Note: The project cannot be exempted.
 FORMCHECKBOX 
 No

	30. Will saw and sander dust generated at this facility be controlled by individual dust collection systems and/or by a shop dust collector with combined control efficiency of 98% or greater for PM10/PM2.5?
	 FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No  Note: The project cannot be exempted.

	RECORDS RETENTION (IDAPA 58.01.01.220.02)

	31.
Unless the source is subject to and the owner or operator complies with Section 385, the owner or operator of the source, except for those sources listed in Subsections 222.02.a. through 222.02.g., shall maintain documentation on site which shall identify the exemption determined to apply to the source and verify that the source qualifies for the identified exemption. The records and documentation shall be kept for a period of time not less than five (5) years from the date the exemption determination has been made or for the life of the source for which the exemption has been determined to apply, which ever is greater, or until such time as a permit to construct or an operating permit is issued which covers the operation of the source. The owner or operator shall submit the documentation to the Department upon request.
Will records be maintained in accordance with IDAPA 58.01.01.222.02?
	 FORMCHECKBOX 
 Yes

 FORMCHECKBOX 

No  Note: The project cannot be exempted.

	CERTIFICATION (IDAPA 58.01.01.123)

	In accordance with IDAPA 58.01.01.123 (Rules for the Control of Air Pollution in Idaho), I certify based on information and belief formed after reasonable inquiry, the statements and information in the document(s) are true, accurate, and complete.

	32. Responsible Official’s Name and Title:
	     

	33. Responsible Official’s Signature:
	
	Dated:      


	Instructions for Form EXPT

	Please refer to IDAPA 58.01.01.220 for a list of the general exemption criteria for Permit to Construct exemptions.


1 – 5.
Provide the company name, facility name (if different), facility ID number (if known), the facility NAICS code (if known), and a brief project description.
USE ATTACHMENTS IF ADDITIONAL SPACE IS REQUIRED.

General Information:

6 – 11.
Provide facility contact information who can answer any questions about the exemption application by DEQ staff as well as the facility address and mailing address for correspondence.

Level I or Level II Exemption:
12.
Specify which exemption type you will use. As noted in the form, a Level I exemption is more broadly tailored and will be the best choice for most facilities. A Level II exemption may be more beneficial if you use coating materials that contain Carbon Black, Chromium, or Silica Quartz.

Level I Exemption:
13.
Specify whether coating usage will exceed 3 gallons per day. Usage in exceedance of this amount disqualifies a facility from this exemption. Note that this amount should not include usage of materials that contain Benzene, Formaldehyde, Carbon Black, Chromium III, or Silica Quartz. Usage of these materials is covered in question 14a.

14a-b.
Specify whether coatings containing Benzene, Formaldehyde, Carbon Black, Chromium III, or Silica Quartz will be used and if so, whether they will be used in amounts greater than those specified.  Any usage exceeding a specified amount will disqualify a facility from this exemption.

15.
Specify whether naphthalene containing coatings are used. Any usage of naphthalene containing coatings disqualifies a facility from this exemption.

16.
Specify whether spray coating activities will occur in an enclosed booth equipped with a filter system capable of achieving 98% control efficiency for PM10/PM2.5. If spray coating activities will occur outside of such a booth, the project cannot be exempted.

17a-b.
Specify whether space heaters, furnaces, or boilers will be used, and if so, what kind of fuels they will burn.

17c-d.
After being directed to the appropriate fuel scenario, specify whether the total heat input will exceed the listed quantity.  Total heat input in excess of these quantities cannot be exempted.

18.
Specify whether a dust control system will be used.  Either individual (tool specific) control systems or a shop-wide system must be used.  In either case, the control efficiency of the system must be 98% or greater.  Lacking such a system, the project cannot be exempted.

Level I Exemption:
19.
Specify whether coating usage will exceed 3 gallons per day. Usage in exceedance of this amount disqualifies a facility from this exemption. Note that this amount should not include usage of materials that contain Benzene, Formaldehyde, Carbon Black, Chromium III, or Silica Quartz. Usage of these materials is covered in question 14a.

20a-b.
Specify whether coatings containing Benzene, Carbon Black, Chromium III, or Silica Quartz will be used and if so, whether they will be used in amounts greater than those specified.  Any usage exceeding a specified amount will disqualify a facility from this exemption.

21. 
Specify whether naphthalene containing coatings are used. Any usage of naphthalene containing coatings disqualifies a facility from this exemption.

22.
Specify whether spray coating activities will occur in an enclosed booth equipped with a filter system capable of achieving 98% control efficiency for PM10/PM2.5. If spray coating activities will occur outside of such a booth, the project cannot be exempted.

23.
Specify whether space heaters, furnaces, or boilers will be used.

24.
If heaters will not be used, specify whether any formaldehyde containing coating materials will be used in excess of 42 gallons per year. If so, the project cannot be exempted.

25.
If space heaters/furnaces/boilers will be used, specify what kind/combination of fuels they will use.

26.
This question pertains only to sources with electric heaters. Specify whether any formaldehyde containing coating materials will be used in excess of 42 gallons per year. If so, the project cannot be exempted.

27a-c.
These questions pertain to sources with natural gas/LPG-fired heaters/furnaces/boilers only. First, specify whether the total heat input for all units exceeds 0.33 MMBtu/hr.  If not, no limits on hours of operation need apply.  If so, specify whether the total heat input exceeds 1.4 MMBtu/hr and whether operation of these heaters will exceed 2,080 hr/yr. If so, the project cannot be exempted.  Finally, specify whether use of formaldehyde containing spray coatings will exceed 21 gallons per year.  If so, the project cannot be exempted.

28a-c.
These questions pertain to sources with diesel heaters/furnaces/boilers only. First, specify whether the total heat input for all units exceeds 0.04 MMBtu/hr.  If not, no limits on hours of operation need apply.  If so, specify whether the total heat input exceeds 0.15 MMBtu/hr and whether operation of these heaters will exceed 2,080 hr/yr. If so, the project cannot be exempted.  Finally, specify whether use of formaldehyde containing spray coatings will exceed 35 gallons per year.  If so, the project cannot be exempted.

29a-c.
These questions pertain to sources with both natural gas/LPG and diesel heaters/furnaces/boilers. First, specify whether the total heat input for all natural gas/LPG-fired units exceeds 0.12 MMBtu/hr and whether the use of all diesel-fired units will exceed 0.03 MMBtu/hr.  If not, no limits on hours of operation need apply. If so, specify whether the total heat input exceeds 0.50 MMBtu/hr for all natural gas/LPG-fired units, whether the total heat input of all diesel-fired units exceeds 0.13 MMBtu/hr, and whether operation of any of these units will exceed 2,080 hr/hr. If so, the project cannot be exempted.  Finally, specify whether use of formaldehyde containing spray coatings will exceed 29 gallons per year.  If so, the project cannot be exempted.

30.
Specify whether a dust control system will be used.  Either individual (tool specific) control systems or a shop-wide system must be used.  In either case, the control efficiency of the system must be 98% or greater.  Lacking such a system, the project cannot be exempted.

Records Retention (IDAPA 58.01.01.220.02):
31.
Specify whether records will be maintained in accordance with IDAPA 58.01.01.222.02.

Certification (IDAPA 58.01.01.123):
32-33.
Provide the name and title of the Responsible Official for the facility. Have the Responsible Official sign and date the form.
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